;; Car Information setup file
;
; - Semi-colons are for comments (up to next new line)
; - Not case sensitive
; - Curly braces delimit information
;

NUMCARS		34		; Number of different car types in the game
 
;================================
; All Cars: Default Safe Values
;
; This sets all the definable
; values on every car to a 
; safe default. Use this as a 
; template if you like...but...
;
;	DO NOT CHANGE
;
;================================

CAR 0-33 {	

	Name		"Right about now"

	; Model Filenames

	MODEL	0		NONE				; Body model
	MODEL	1		NONE				; wheel front left
	MODEL	2		NONE				; wheel front right
	MODEL	3		NONE				; wheel back left
	MODEL	4		NONE				; wheel back right
	MODEL	5		NONE				; spring front left
	MODEL	6		NONE				; spring front right
	MODEL	7		NONE				; spring back left
	MODEL	8		NONE				; spring back right
	MODEL	9		NONE				; axle front left
	MODEL	10		NONE				; axle front right
	MODEL	11		NONE				; axle back left
	MODEL	12		NONE				; axle back right
	MODEL	13		NONE				; pin front left
	MODEL	14		NONE				; pin front right
	MODEL	15		NONE				; pin back left
	MODEL	16		NONE				; pin back right
	MODEL	17		NONE				; Aerial section
	MODEL	18		NONE				; Aerial Top

	TPAGE	NONE

	COLL	NONE

	EnvRGB	255 255 255
	
	SteerRate		2.5 ;3.0
	SteerMod		0.4 ;0.5
	EngineRate		4.5
	TopSpeed		45.0
	MaxRevs			0.5
	DownForceMod	2.0

	CoM				0.0 0.0 0.0

	BestTime		TRUE
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0
	TOPEND		50
	ACC			50
	WEIGHT		50
	HANDLING		50
	TRANS			0

	Weapon			0.0 -32.0, 64.0

	; Body

	BODY {
		MODELNUM	-1,							; Model Number
		OFFSET		0, 0, 0,
		MASS		1.0f,						; Mass
		INERTIA		870, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1250, 0.0f, 
					0.0f, 0.0f, 440,
		GRAVITY		2200.0f,					; Acc due to gravity
		HARDNESS	0.0f,						; Hardness
		RESISTANCE	0.001f,						; Air resistance
		ANGRES		0.001f,						; Angular Air resistance
		RESMOD		25.0f,						; increase in ang resistance when in air
		GRIP		0.01,
		STATICFRICTION	0.8f,					; Static Friction
		KINETICFRICTION	0.4f,					; Kinetic Friction
	}

	; Shared wheel Attributes

	WHEEL 0 - 3 {
		IsPresent	Yes
		RADIUS		10
		MASS		0.2							; Mass
		GRAVITY		2200.0f						; Gravity
		MaxPos		8.0
		ENGINERATIO		5000					; Engine Ratio
		Grip			0.018
		SkidWidth		10.0
		ToeIn				0.0
	}		

	; Individual Wheel Attributes

	WHEEL 0 {
		MODELNUM	-1
		OFFSET1		-16, 14, 32, 
		OFFSET2		-4.5, 0, 0,
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		AXLEFRICTION	0.02f					; Axle Friction
		STATICFRICTION	1.58f					; Static Friction
		KINETICFRICTION	1.10f					; Kinetic Friction
	}

	WHEEL 1 {
		MODELNUM	-1
		OFFSET1		16, 14, 32, 
		OFFSET2		4.5, 0, 0,
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		AXLEFRICTION	0.02f					; Axle Friction
		STATICFRICTION	1.58f					; Static Friction
		KINETICFRICTION	1.10f					; Kinetic Friction
	}

	WHEEL 2 {
		MODELNUM	-1
		OFFSET1		-16, 14, -38, 
		OFFSET2		-6, 0, 0,
		IsTurnable	FALSE
		SteerRatio	0.1
		IsPowered	TRUE
		AXLEFRICTION	0.05f					; Axle Friction
		STATICFRICTION	1.53f					; Static Friction
		KINETICFRICTION	1.09f					; Kinetic Friction
	}

	WHEEL 3 {
		MODELNUM	-1
		OFFSET1		16, 14, -38, 
		OFFSET2		6, 0, 0,
		IsTurnable	FALSE
		SteerRatio	0.1
		IsPowered	TRUE
		AXLEFRICTION	0.05f					; Axle Friction
		STATICFRICTION	1.53f					; Static Friction
		KINETICFRICTION	1.09f					; Kinetic Friction
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	250.0
		Damping		7.0
		Restitution	-0.85
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	SPINNER {
		MODELNUM	-1
		OFFSET		0, 0, 0
		AXIS		0, 1, 0
		ANGVEL		0	
	}

	AERIAL {
		SECMODELNUM	-1
		TOPMODELNUM -1
		OFFSET		12, -33, -27,
		DIRECTION	0, -1, 0
		LENGTH		13
		STIFFNESS	2000
		DAMPING		5.5
	}
}


;=====================================
;
;Individual details - change these
;
;=====================================


;/////////////////////////////////////////////////////////////////////
;//
;// Starting Cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 0: RC Bandit
;=====================================
Car 0 {

	Name			"RC Bandit"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0
	TOPEND		32
	ACC			55
	HANDLING		90

	EnvRGB	200 200 200

	TPAGE			"cars\rc\car.bmp"

	COLL			"cars\rc\hull.hul"

	MODEL	0		"cars\rc\body.prm"			; Body model
	MODEL	1		"cars\rc\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\rc\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\rc\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\rc\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\rc\spring.prm"		; all springs

	MODEL	9		"cars\rc\axle.prm"			; all axles
	MODEL	13		"cars\rc\pin.prm"			; all pins

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top



	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-18, 7, 42,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		18, 7, 42,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-18, 9, -42,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		18, 9, -42,
	}

	SPRING 0 {
		MODELNUM	5
		OFFSET		-6, -10, 41
		LENGTH		16
	}
	SPRING 1 {
		MODELNUM	5
		OFFSET		6, -10, 41
		LENGTH		16
	}
	SPRING 2 {
		MODELNUM	5
		OFFSET		-8, -12, -38,
		LENGTH		16
	}
	SPRING 3 {
		MODELNUM	5
		OFFSET		8, -12, -38,
		LENGTH		16
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-7, 7, 42,
		LENGTH		12
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		7, 7, 42,
		LENGTH		12
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-7, 7, -30,
		LENGTH		12
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		7, 7, -30,
		LENGTH		12
	}

	PIN	0 {
		MODELNUM	13
		OFFSET		0, 0, 0
		LENGTH		-1.35
	}
	PIN	1 {
		MODELNUM	13
		OFFSET		0, 0, 0
		LENGTH		-1.35
	}
		

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-5, -6, -30
		LENGTH		20
	}


	CoM		0.0 -5.0 1.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		33.5

	BODY {
		MASS		1.2f,						; Mass
		INERTIA	1050, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1200, 0.0f, 
					0.0f, 0.0f, 300,	
		RESMOD	30.0
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	6500

		RADIUS		10
		MASS		0.15						; Mass
		STEERRATIO	-0.5f						; Steer Ratio
		STATICFRICTION	1.5					; Static Friction
		KINETICFRICTION	1.45					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	6500

		RADIUS		10
		MASS		0.15						; Mass
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.5					; Static Friction
		KINETICFRICTION	1.45					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0-1 {
		Stiffness	300.0
		Damping		7.0
		Restitution	-0.95
	}
	SPRING 2-3 {
		Stiffness	300.0
		Damping		7.0
		Restitution	-0.95
	}

}	

;=====================================
; Car 1: dust mite
;=====================================
Car 1 {

	Name			"Dust Mite"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0

	EnvRGB	200 100 200

	TPAGE			"cars\mite\car.bmp"

	COLL			"cars\mite\hull.hul"

	MODEL	0		"cars\mite\body.prm"		; Body model
	MODEL	1		"cars\mite\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\mite\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\mite\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\mite\wheelbr.prm"		; wheel back right
        MODEL   5               "cars\mite\spring.prm"          ; springs
	MODEL	9		"cars\mite\axle.prm"		; all axles

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-20, 2, 37,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		20, 2, 37,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-23, 5, -32
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		23, 5, -32
	}

	SPRING 0 {
		MODELNUM	5
		OFFSET		-10, -10, 32
		LENGTH		15
	}
	SPRING 1 {
		MODELNUM	5
		OFFSET		10, -10, 32
		LENGTH		15
	}
	SPRING 2 {
		MODELNUM	5
		OFFSET		-12, -12, -26
		LENGTH		15
	}
	SPRING 3 {
		MODELNUM	5
		OFFSET		12, -12, -26
		LENGTH		15
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-7, 0, 35
		LENGTH		9
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		7, 0, 35
		LENGTH		9
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-8, -1, -28
		LENGTH		9
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		8, -1, -28
		LENGTH		9
	}
	
	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		14, -4, -10
		LENGTH		30
	}

	TopSpeed		33.0
	CoM			0.0 -3.0 -5.0

	BODY {
		MODELNUM	0
		MASS		1.2f,						; Mass
		INERTIA	780, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 980, 0.0f, 
					0.0f, 0.0f, 300,	
	}

	WHEEL 0-1 {
		StaticFriction	1.50
		KineticFriction	1.35
		Radius			11.0
		Grip			0.015
		MaxPos			10.0
		Engineratio	7000
		IsPowered	TRUE
	}

	WHEEL 2-3 {
		StaticFriction	1.50
		KineticFriction	1.35
		Radius			12.0
		MaxPos			10.0
		Grip			0.018
		IsPowered	TRUE
		Engineratio	7000
	}

	SPRING 0-1 {
		Stiffness	380 ;400
		Damping		9.0 ;12.0
		Restitution	-0.95 ;-0.85
	}

	SPRING 2-3 {
		Stiffness	380 ;380
		Damping		9.0 ;11.5
		Restitution	-0.95 ;-0.85
	}
}	

;=====================================
; Car 2: Phat Slag
;=====================================
Car 2 {

	Name			"Phat Slug"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0


	EnvRGB	0 200 0

	TPAGE			"cars\phat\car.bmp"

	COLL			"cars\phat\hull.hul"

	MODEL	0		"cars\phat\body.prm"		; Body model
	MODEL	1		"cars\phat\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\phat\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\phat\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\phat\wheelbr.prm"		; wheel back right

	MODEL	5		"cars\phat\spring.prm"		; all springs
	MODEL	9		"cars\phat\axle.prm"		; all axles

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0-3 {
		Radius		12.8
		SkidWidth	18.0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-25, 0, 37,
		OFFSET2		-9, 0, 0,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		25, 0, 37,
		OFFSET2		9, 0, 0,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-25, 0, -47
		OFFSET2		-9, 0, 0,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		25, 0, -47
		OFFSET2		9, 0, 0,
	}

	SPRING 0 {
		MODELNUM	5
		OFFSET		-13, -16, 34
		LENGTH		6.7
	}
	SPRING 1 {
		MODELNUM	5
		OFFSET		13, -16, 34
		LENGTH		6.7
	}
	SPRING 2 {
		MODELNUM	5
		OFFSET		-12, -28, -44
		LENGTH		6.7
	}
	SPRING 3 {
		MODELNUM	5
		OFFSET		12, -28, -44
		LENGTH		6.7
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-7, -2, 35
		LENGTH		12
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		7, -2, 35
		LENGTH		12
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-7, -4, -47
		LENGTH		12
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		7, -4, -47
		LENGTH		12
	}
	
	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-20, -28, -28
		DIRECTION	-0.31, -0.9, -0.31
		LENGTH		20
	}

	CoM			0.0 -4.0 -3.0
	TopSpeed		35.0

	Spring 0-1 {
		Stiffness		700.0
		Damping			10
		Restitution		-0.95
	}	
	Spring 2-3 {
		Stiffness		700.0
		Damping			10
		Restitution		-0.95
	}	
	BODY {
		MODELNUM	0
		MASS		2.5
		INERTIA	3300, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 3900, 0.0f, 
					0.0f, 0.0f, 1400,	
	}

	Wheel 0-1 {
		radius	16.0
		IsPowered	FALSE
		IsTurnable	TRUE
		SteerRatio	-0.45

		MASS			0.4						; Mass
		MaxPos		15.0
		SkidWidth		20.0
		STATICFRICTION	1.8					; Static Friction
		KINETICFRICTION	1.75					; Kinetic Friction
		Grip		0.016
	}

	Wheel 2-3 {
		radius	18.0
		EngineRatio	30000

		MASS			0.4						; Mass
		MaxPos		15.0
		SkidWidth		20.0
		STATICFRICTION	1.90					; Static Friction
		KINETICFRICTION	1.85					; Kinetic Friction
		Grip		0.016
	}
}	

;=====================================
; Car 3: Col. moss
;=====================================
Car 3 {

	Name			"Col. Moss"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0

	EnvRGB  100 200 100

	TPAGE			"cars\moss\car.bmp"

	COLL			"cars\moss\hull.hul"

	MODEL	0		"cars\moss\body.prm"		; Body model
	MODEL	1		"cars\moss\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\moss\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\moss\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\moss\wheelbr.prm"		; wheel back right

	MODEL	9		"cars\moss\axle.prm"		; all axles

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top


	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-20, -5, 39,
		radius          9
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		20, -5, 39,
		radius          9
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-20, -5, -45
		radius          9
        }
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		20, -5, -45
		radius          9
        } 

	AXLE 0 {
		MODELNUM	9
		OFFSET		0, -4, 30
		LENGTH		20
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		0, -4, 30
		LENGTH		20
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		0, -4, -36
		LENGTH		20
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		0, -4, -36
		LENGTH		20
	}
	
	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-10, -24, -40
		LENGTH		20
	}

	CoM		0.0 10.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		34.0

	BODY {
		MASS		1.5f,						; Mass
		INERTIA	1175, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1520, 0.0f, 
					0.0f, 0.0f, 493,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	8500

		RADIUS		10
		MASS		0.15						; Mass
		STEERRATIO	-0.3f						; Steer Ratio
		STATICFRICTION	1.30					; Static Friction
		KINETICFRICTION	1.18					; Kinetic Friction
		Grip		0.013
		SkidWidth	13.0
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	8500

		RADIUS		10
		MASS		0.15						; Mass
		STATICFRICTION	1.30					; Static Friction
		KINETICFRICTION	1.18					; Kinetic Friction
		Grip		0.014
		SkidWidth	13.0
	}

	SPRING 0-1 {
		Stiffness	500.0
		Damping		12.0
		Restitution	-0.8
	}
	SPRING 2-3 {
		Stiffness	460.0
		Damping		10.0
		Restitution	-0.8
	}

}	


;=====================================
; Car 4: Harvester
;=====================================
Car 4 {

	Name			"Harvester"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0

	EnvRGB	200 200 0

	TPAGE			"cars\mud\car.bmp"

	COLL			"cars\mud\hull.hul"

	MODEL	0		"cars\mud\body.prm"		; Body model
	MODEL	1		"cars\mud\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\mud\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\mud\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\mud\wheelbr.prm"		; wheel back right
	MODEL	9		"cars\mud\axle.prm"		; axle

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-21, -12, 39,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1	    21, -12, 39,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-22.5, -9, -31
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		22.5, -9, -31
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		0, -15, 39
		LENGTH		20
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		0, -15, 39
		LENGTH		18
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		0, -15, -38
		LENGTH		18
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		0, -15, -38
		LENGTH		18
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-9, -33, -27
		LENGTH		34
	}
	
	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		30


	CoM		0.0, 9.0, -5.0

	BODY {
		MODELNUM	0
		MASS		1.7f,						; Mass
		INERTIA	1655, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1890, 0.0f, 
					0.0f, 0.0f, 715,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	16500

		RADIUS		15.5
		MASS			0.15						; Mass
		MaxPos		12.0
		STEERRATIO	-0.4f						; Steer Ratio
		STATICFRICTION	1.85					; Static Friction
		KINETICFRICTION	1.80					; Kinetic Friction
		Grip		0.017
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	16500

		RADIUS		16.0
		MASS			0.15					; Mass
		MaxPos		12.0
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.82					; Static Friction
		KINETICFRICTION	1.77					; Kinetic Friction
		Grip		0.017
	}
	SPRING 0-1 {
		Stiffness		300.0
		Damping		3.5
		Restitution 	-0.95
	}
	SPRING 2-3 {
		Stiffness		250.0
		Damping		3.0
		Restitution 	-0.95
	}

}	

;=====================================
; Car 5:doc grudge
;=====================================
Car 5 {

	EnvRGB  200 200 200

	Name			"Dr. Grudge"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0

	TPAGE			"cars\beatall\car.bmp"

	COLL			"cars\beatall\hull.hul"

	MODEL	0		"cars\beatall\body.prm"		; Body model
	MODEL	1		"cars\beatall\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\beatall\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\beatall\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\beatall\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\beatall\spring.prm"		; springs

	MODEL	9		"cars\beatall\axle.prm"		; all axles

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-24, -1, 37,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		24, -1, 37,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-24, 1, -36
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		24, 1, -36
	}

	SPRING 0 {
		MODELNUM	5
		OFFSET		-12, -20, 34
		LENGTH		22
	}
	SPRING 1 {
		MODELNUM	5
		OFFSET		12, -20, 34
		LENGTH		22
	}
	SPRING 2 {
		MODELNUM	5
		OFFSET		-12, -19, -33
		LENGTH		19
	}
	SPRING 3 {
		MODELNUM	5
		OFFSET		12, -19, -33
		LENGTH		19
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		0, -1, 35
		LENGTH		18
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		0, -1, 35
		LENGTH		18
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		0, -3, -28
		LENGTH		18
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		0, -3, -28
		LENGTH		18
	}
	
	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-10, -22, -30
		LENGTH		35
	}

	CoM		0.0 2.0 -4.0

	SteerRate	3.0
	SteerMod		0.4
	EngineRate	4.5
	TopSpeed		32.0

	BODY {
		MASS		1.4f,						; Mass
		INERTIA	780, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1015, 0.0f, 
					0.0f, 0.0f, 445,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	12000
		MaxPos		12.0

		RADIUS		12
		MASS		0.15						; Mass
		STEERRATIO	-0.5f						; Steer Ratio
		STATICFRICTION	1.50					; Static Friction
		KINETICFRICTION	1.5					; Kinetic Friction
		Grip		0.014
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	12000
		MaxPos		12.0

		RADIUS		13
		MASS		0.15						; Mass
		STATICFRICTION	1.50					; Static Friction
		KINETICFRICTION	1.5					; Kinetic Friction
		Grip		0.014
	}

	SPRING 0-1 {
		Stiffness	400.0
		Damping		9
		Restitution	-0.95
	}
	SPRING 2-3 {
		Stiffness	400.0
		Damping		9
		Restitution	-0.95
	}


}	

;=====================================
; Car 6: Volken
;=====================================
Car 6 {

	EnvRGB			200 200 200

	Name			"Volken Turbo"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0

	TPAGE			"cars\Volken\Volken.bmp"
	COLL			"cars\Volken\hull.hul"

	MODEL	0		"cars\Volken\body.prm"			; Body model
	MODEL	1		"cars\Volken\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\Volken\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\Volken\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\Volken\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-25.5, -4, 41,
		OFFSET2		-2.5, 0, 0,
		SkidWidth	10
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		25.5, -4, 41,
		OFFSET2		2.5, 0, 0,
		SkidWidth	10
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-27, -4, -39,
		OFFSET2		-2, 0, 0,
		SkidWidth	11
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		27, -4, -39,
		OFFSET2		2, 0, 0,
		SkidWidth	11
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-17, -22, -45
		LENGTH		17
	}


	CoM		0.0 5.0 -10.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		33.0

	BODY {
		MASS		1.6f,						; Mass
		INERTIA	2600, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 3010, 0.0f, 
					0.0f, 0.0f, 750,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	21000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		7.0
		STATICFRICTION	1.6					; Static Friction
		KINETICFRICTION	1.45					; Kinetic Friction
		Grip		0.020
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	FALSE
		EngineRatio	10000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		7.0
		STATICFRICTION	1.6					; Static Friction
		KINETICFRICTION	1.45					; Kinetic Friction
		Grip		0.020
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	700.0
		Damping		12.0
		Restitution	-0.95
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;=====================================
; Car 7: Sprinter XL
;=====================================
Car 7 {

	EnvRGB			200 200 200

	Name			"Sprinter XL"
	Selectable		TRUE
	CLASS			0
	OBTAIN		0
	RATING		0
	TOPEND		31
	ACC			70
	HANDLING		80

	TPAGE			"cars\tc6\car.bmp"

	COLL			"cars\tc6\hull.hul"

	MODEL	0		"cars\tc6\body.prm"			; Body model
	MODEL	1		"cars\tc6\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\tc6\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\tc6\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\tc6\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-19.5, -3, 31,
		OFFSET2		-2, 0, 0
		SkidWidth	14
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		19.5, -3, 31,
		OFFSET2		2, 0, 0
		SkidWidth	14
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-20, -3, -39,
		OFFSET2		-2, 0, 0
		SkidWidth	14
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		20, -3, -39,
		OFFSET2		2, 0, 0
		SkidWidth	14
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		20, -17, 21
		LENGTH		17
		DAMPING		2.5
	}


	;CoM		0.0 2.0 6.0
	CoM		0.0 2.0 -2.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		30.5

	BODY {
		MASS		0.9f,						; Mass
		INERTIA	1344, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1550, 0.0f, 
					0.0f, 0.0f, 365,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	9500

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STEERRATIO	-0.4f						; Steer Ratio
		STATICFRICTION	1.55					; Static Friction
		KINETICFRICTION	1.35					; Kinetic Friction
		Grip		0.014
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	8500

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.55					; Static Friction
		KINETICFRICTION	1.35					; Kinetic Friction
		Grip		0.014
	}

	SPRING 0 - 1 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	1000.0
		Damping		15.0
		Restitution	-0.85
	}

	SPRING 2 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	800.0
		Damping		12.0
		Restitution	-0.85
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;/////////////////////////////////////////////////////////////////////
;//
;// Bronze cup cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 8: Dynamo San
;=====================================
Car 8 {

	Name			"Dynamo San"
	Selectable		TRUE
	CLASS			0
	OBTAIN		1
	RATING		1

	EnvRGB	0	64	200

	TPAGE			"cars\dino\dino.bmp"

	COLL			"cars\dino\hull.hul"

	MODEL	0		"cars\dino\body.prm"		; Body model
	MODEL	1		"cars\dino\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\dino\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\dino\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\dino\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\dino\spring.prm"

	MODEL	9		"cars\dino\axle.prm"		; all axles

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-22, 0, 29,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		22, 0, 29,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-23, 0, -36
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		23, 0, -36
	}

	SPRING 0 {
		MODELNUM	5
		OFFSET		-15, -8, 28
		LENGTH		4
	}
	SPRING 1 {
		MODELNUM	5
		OFFSET		15, -8, 28
		LENGTH		4
	}
	SPRING 2 {
		MODELNUM	5
		OFFSET		-17, -8, -36
		LENGTH		4
	}
	SPRING 3 {
		MODELNUM	5
		OFFSET		17, -8, -36
		LENGTH		4
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-18, 0, 30
		LENGTH		12
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		18, 0, 30
		LENGTH		12
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-18, 0, -33
		LENGTH		16
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		18, 0, -33
		LENGTH		12
	}
	
	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		0, -15, -40
		LENGTH		25
	}

	CoM				0.0 3.0 -4.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		32.0

	BODY {
		MASS		1.0f,						; Mass
		INERTIA	890, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1150, 0.0f, 
					0.0f, 0.0f, 370,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	8000

		RADIUS		10
		MASS		0.15						; Mass
		STATICFRICTION	1.40					; Static Friction
		KINETICFRICTION	1.35					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	10000

		RADIUS		10
		MASS		0.15						; Mass
		STATICFRICTION	1.45					; Static Friction
		KINETICFRICTION	1.40					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0-1 {
		Stiffness	500.0
		Damping		12.0
		Restitution	-0.8
	}
	SPRING 2-3 {
		Stiffness	460.0
		Damping		10.0
		Restitution	-0.8
	}

}	

;=====================================
; Car 9: candy pebbles
;=====================================
Car 9 {

	Name			"Candy Pebbles"
	Selectable		TRUE
	CLASS			0
	OBTAIN		1
	RATING		1

	EnvRGB	255 255 255

	TPAGE			"cars\candy\car.bmp"

	COLL			"cars\candy\candy.hul"

	MODEL	0		"cars\candy\body.prm"		; Body model
	MODEL	1		"cars\candy\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\candy\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\candy\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\candy\wheelbr.prm"		; wheel back right
	MODEL	9		"cars\candy\axle.prm"		; axle
	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-22, -6, 32,
		OFFSET2		-9, 0, 0
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1	    	22, -6, 32,
		OFFSET2		9, 0, 0
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-22, -6, -34
		OFFSET2		-9, 0, 0
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		22, -6, -34
		OFFSET2		9, 0, 0
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		0, -15, 39
		LENGTH		20
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		0, -15, 39
		LENGTH		18
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		0, -15, -38
		LENGTH		18
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		0, -15, -38
		LENGTH		18
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-11, -28, -27
		LENGTH		34
	}
	
	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		35.5

	CoM		0.0 5.0 0.0

	BODY {
		MODELNUM	0
		MASS		1.3f,						; Mass
		INERTIA	1220, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1555, 0.0f, 
					0.0f, 0.0f, 612	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	FALSE
		EngineRatio	10000
		SkidWidth	18.0

		RADIUS		12.5
		MASS			0.15						; Mass
		STATICFRICTION	1.85					; Static Friction
		KINETICFRICTION	1.80					; Kinetic Friction
		Grip		0.020
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	15000
		SkidWidth	18.0

		RADIUS		12.5
		MASS			0.15					; Mass
		STATICFRICTION	1.82					; Static Friction
		KINETICFRICTION	1.77					; Kinetic Friction
		Grip		0.020
	}
	SPRING 0-1 {
		Stiffness		400.0
		Damping		3.0
		Restitution 	-0.8
	}
	SPRING 2-3 {
		Stiffness		350.0
		Damping		3.0
		Restitution 	-0.8
	}

}	


;/////////////////////////////////////////////////////////////////////
;//
;// Bronze practise cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 10: genghis Khar
;=====================================
Car 10 {

	Name			"Genghis Kar"
	Selectable		TRUE
	CLASS			0
	OBTAIN		3
	RATING		1


	EnvRGB 200 0 0

	TPAGE			"cars\gencar\car.bmp"

	COLL			"cars\gencar\hull.hul"

	MODEL	0		"cars\gencar\body.prm"		; Body model
	MODEL	1		"cars\gencar\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\gencar\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\gencar\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\gencar\wheelbr.prm"		; wheel back right
    MODEL   5		"cars\gencar\spring.prm"                ; springs
	MODEL	9		"cars\gencar\axle.prm"		; all axles

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	CoM			0.0 2.0 0.0

	BODY {
		MODELNUM	0
	}

	WHEEL 0-1 {
		SkidWidth	10.0
	}
	WHEEL 2-3 {
		SkidWidth	18.0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-25, 4.7, 35,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		25, 4.7, 35,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-24, 4.7, -38
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		24, 4.7, -38
	}

	SPRING 0 {
		MODELNUM	5
		OFFSET		-14, -5, 25
		LENGTH		30
	}
	SPRING 1 {
		MODELNUM	5
		OFFSET		14, -5, 25
		LENGTH		30
	}
	SPRING 2 {
		MODELNUM	5
		OFFSET		-13, -5, -33
		LENGTH		30
	}
	SPRING 3 {
		MODELNUM	5
		OFFSET		13, -5, -33
		LENGTH		30
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-13, 2, 35
		LENGTH		12
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		13, 2, 35
		LENGTH		12
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-13, 1, -36
		LENGTH		12
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		13, 1, -36
		LENGTH		12
	}
	
	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-16, -11, -25
		LENGTH		20
	}


	TopSpeed	40.0

	BODY {
		MODELNUM	0
		MASS		2.0f,						; Mass
		INERTIA	2830, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 3270, 0.0f, 
					0.0f, 0.0f, 970,
		ResMod		20.0
	}

	WHEEL 0-1 {
		StaticFriction	1.45
		KineticFriction	1.35
		Radius			13.5
		Grip			0.014
		MaxPos			10.0
		IsPowered	TRUE
		Engineratio	11000
		IsTurnable	TRUE
		SteerRatio	-0.35
	}

	WHEEL 2-3 {
		StaticFriction	1.45
		KineticFriction	1.35
		Radius			13.5
		MaxPos			10.0
		Grip			0.014
		IsPowered	TRUE
		Engineratio	11000
		IsTurnable	TRUE
		SteerRatio	0.03
	}

	SPRING 0-1 {
		Stiffness	400
		Damping		5.0
		Restitution	-0.9
	}

	SPRING 2-3 {
		Stiffness	380
		Damping		4.5
		Restitution	-0.8
	}
}	

;=====================================
; Car 11: Aquasonic
;=====================================
Car 11 {

	EnvRGB			200 200 200

	Name			"Aquasonic"
	Selectable		TRUE
	CLASS			1
	OBTAIN		3
	RATING		1

	TPAGE			"cars\tc4\car.bmp"

	COLL			"cars\tc4\hull.hul"

	MODEL	0		"cars\tc4\body.prm"			; Body model
	MODEL	1		"cars\tc4\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\tc4\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\tc4\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\tc4\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-23.5, -3, 34,
		OFFSET2		-2, 0, 0
		SkidWidth	14
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		23.5, -3, 34,
		OFFSET2		2, 0, 0
		SkidWidth	14
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-25, -3, -44,
		OFFSET2		-2, 0, 0
		SkidWidth	14
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		25, -3, -44,
		OFFSET2		2, 0, 0
		SkidWidth	14
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		23, -20, -52
		LENGTH		17
	}


	CoM		0.0 2.0 10.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		33.0

	BODY {
		MASS		1.4f,						; Mass
		INERTIA	1400, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2200, 0.0f, 
					0.0f, 0.0f, 700,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	FALSE

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.6				; Static Friction
		KINETICFRICTION	1.5				; Kinetic Friction
		Grip		0.016
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	20000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.65					; Static Friction
		KINETICFRICTION	1.55					; Kinetic Friction
		Grip		0.016
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	600.0
		Damping		10.0
		Restitution	-0.85
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;/////////////////////////////////////////////////////////////////////
;//
;// Bronze single race cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 12: Mouse
;=====================================
Car 12 {

	Name			"Mouse"
	Selectable		TRUE
	CLASS			0
	OBTAIN		4
	RATING		1

	EnvRGB			200 200 200

	TPAGE			"cars\mouse\car.bmp"

	COLL			"cars\mouse\hull.hul"

	MODEL	0		"cars\mouse\body.prm"		; Body model
	MODEL	1		"cars\mouse\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\mouse\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\mouse\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\mouse\wheelbr.prm"		; wheel back right
	MODEL	9		"cars\mouse\axle.prm"		; axle

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	CoM		0.0 10.0 -5.0

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-30, 3, 39,
		OFFSET2		-8, 0, 0,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1	    	30, 3, 39,
		OFFSET2		8, 0, 0,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-30, 3, -38
		OFFSET2		-8, 0, 0,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		30, 3, -38
		OFFSET2		8, 0, 0,
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-3, -2, 35
		LENGTH		22
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		3, -2, 35
		LENGTH		22
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-3, -1, -36
		LENGTH		22
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		3, -1, -36
		LENGTH		22
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		0, -49, 0
		LENGTH		20
	}

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		10.0
	TopSpeed		33.5

	CoM		0.0, 2.0, 0.0

	BODY {
		MODELNUM	0
		MASS		2.3,						; Mass
		INERTIA	2700, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2680, 0.0f, 
					0.0f, 0.0f, 1480,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	35000

		RADIUS		18.5
		MASS			0.45						; Mass
		MaxPos		20.0
		SkidWidth		23.0
		STATICFRICTION	1.55					; Static Friction
		KINETICFRICTION	1.30					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	35000

		RADIUS		18.5
		MASS			0.45				; Mass
		MaxPos		20.0
		SkidWidth		23.0
		STATICFRICTION	1.50					; Static Friction
		KINETICFRICTION	1.30					; Kinetic Friction
		Grip		0.015
	}
	SPRING 0-1 {
		Stiffness		450.0
		Damping		9.2
		Restitution 	-0.95
	}
	SPRING 2-3 {
		Stiffness		450.0
		Damping		9.2
		Restitution 	-0.95
	}
}	


;/////////////////////////////////////////////////////////////////////
;//
;// Silver cup cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 13: Evil Weasel
;=====================================

Car 13 {

	Name			"Evil Weasel"
	Selectable		TRUE
	CLASS			0
	OBTAIN		1
	RATING		2

	EnvRGB	0 200 200

	TPAGE			"cars\flag\car.bmp"

	COLL			"cars\flag\hull.hul"

	MODEL	0		"cars\flag\body.prm"		; Body model
	MODEL	1		"cars\flag\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\flag\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\flag\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\flag\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\flag\spring.prm"		; all springs

	MODEL	9		"cars\flag\axle.prm"		; all axles
	MODEL	13		"cars\flag\pin.prm"		; all pins

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-20, 3, 46,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		20, 3, 46,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-20, 6.5, -34
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		20, 6.5, -34
	}

	SPRING 0 {
		MODELNUM	5
		OFFSET		-7, -15, 41
		LENGTH		16
	}
	SPRING 1 {
		MODELNUM	5
		OFFSET		7, -15, 41
		LENGTH		16
	}
	SPRING 2 {
		MODELNUM	5
		OFFSET		-11, -22, -38
		LENGTH		16
	}
	SPRING 3 {
		MODELNUM	5
		OFFSET		11, -22, -38
		LENGTH		16
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-7, 3, 46
		LENGTH		12
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		7, 3, 46
		LENGTH		12
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-11, 3, -34
		LENGTH		12
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		11, 3, -34
		LENGTH		12
	}
	
	PIN 0 {
		MODELNUM	13
		OFFSET		0, 0, 0
		LENGTH		-1.5
	}
	PIN 1 {
		MODELNUM	13
		OFFSET		0, 0, 0
		LENGTH		-1.5
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-15, -4, -18
		LENGTH		32
	}

	CoM				0.0 -2.0 -0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		39.5

	BODY {
		MASS		1.4f,						; Mass
		INERTIA		1500, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2200, 0.0f, 
					0.0f, 0.0f, 770,	
		ANGRES		0.005f,						; Angular Air resistance
		RESMOD		10.0f,						; increase in ang resistance when in air
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	7000

		RADIUS		10
		MASS		0.15						; Mass
		STEERRATIO	-0.4f						; Steer Ratio
		STATICFRICTION	1.40					; Static Friction
		KINETICFRICTION	1.15					; Kinetic Friction
		Grip		0.013
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	7000

		RADIUS		10
		MASS		0.15						; Mass
		STATICFRICTION	1.40					; Static Friction
		KINETICFRICTION	1.15					; Kinetic Friction
		Grip		0.013
	}

	SPRING 0-1 {
		Stiffness	350.0
		Damping		3.0
		Restitution	-0.90
	}
	SPRING 2-3 {
		Stiffness	320.0
		Damping		2.8
		Restitution	-0.90
	}

}	


;=====================================
; Car 14: Panga
;=====================================
Car 14 {

	EnvRGB			200 200 200

	Name			"Panga"
	Selectable		TRUE
	CLASS			1
	OBTAIN		1
	RATING		2

	TPAGE			"cars\tc2\car.bmp"
	COLL			"cars\tc2\hull.hul"

	MODEL	0		"cars\tc2\body.prm"			; Body model
	MODEL	1		"cars\tc2\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\tc2\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\tc2\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\tc2\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-21, 2, 29,
		OFFSET2		-2, 0, 0
		SkidWidth	13
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		21, 2, 29,
		OFFSET2		2, 0, 0
		SkidWidth	13
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-21, 2, -44.5,
		OFFSET2		-2, 0, 0
		SkidWidth	13
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		21, 2, -44.0,
		OFFSET2		2, 0, 0
		SkidWidth	13
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		17, -24, -45
		LENGTH		17
	}


	CoM		0.0 0.0 15.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		37.5

	BODY {
		MASS		1.8f,						; Mass
		INERTIA		1500, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2000, 0.0f, 
					0.0f, 0.0f, 800,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	FALSE

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		6.0
		STATICFRICTION	1.6					; Static Friction
		KINETICFRICTION	1.6					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	22000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		6.0
		STATICFRICTION	1.6					; Static Friction
		KINETICFRICTION	1.6					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	800.0
		Damping		9.0
		Restitution	-0.95
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;/////////////////////////////////////////////////////////////////////
;//
;// Silver practise mode cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 15: R6 Turbo
;=====================================
Car 15 {

	Name			"R6 Turbo"
	Selectable		TRUE
	CLASS			1
	OBTAIN		3
	RATING		2

	EnvRGB	200 200 200

	TPAGE			"cars\r5\car.bmp"

	COLL			"cars\r5\hull.hul"

	MODEL	0		"cars\r5\body.prm"		; Body model
	MODEL	1		"cars\r5\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\r5\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\r5\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\r5\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\Aerialt.m"		; Aerial Top

	COM		0.0 -15.0 -8.0
	TopSpeed	40

	BODY {
		MODELNUM	0
		MASS		0.8f,						; Mass
		INERTIA		900, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1250, 0.0f, 
					0.0f, 0.0f, 400,	
	}

	WHEEL 0-1 {
		Radius			12
		STATICFRICTION	1.65
		KINETICFRICTION	1.5
		ENGINERATIO		13000
		Grip			0.015
	}
	WHEEL 2-3 {
		Radius			12
		STATICFRICTION	1.65
		KINETICFRICTION	1.5
		Grip			0.015
		IsPowered	FALSE
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-14, 14, 32.5, 
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		14, 14, 32.5, 
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-13, 14, -38, 
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		13, 14, -38, 
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 	18
		OFFSET		12.0 -19.0 -20.0
		DIRECTION	0.0 -1.0 0.0 ;-0.866 -0.5
	}

	SPRING 0-1 {
		Stiffness	500.0
		Damping		6.0
		Restitution -0.8
	}
	SPRING 2-3 {
		Stiffness	500.0
		Damping		6.0
		Restitution -0.8
	}
}	

;=====================================
; Car 16: Loaded Chique
;=====================================
Car 16 {

	EnvRGB			200 200 200

	Name			"Loaded Chique"
	Selectable		TRUE
	CLASS			1
	OBTAIN		3
	RATING		2

	TPAGE			"cars\tc5\car.bmp"

	COLL			"cars\tc5\hull.hul"

	MODEL	0		"cars\tc5\body.prm"			; Body model
	MODEL	1		"cars\tc5\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\tc5\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\tc5\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\tc5\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-19.5, -3, 31,
		OFFSET2		-2, 0, 0
		SkidWidth	14
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		19.5, -3, 31,
		OFFSET2		2, 0, 0
		SkidWidth	14
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-20, -3, -39,
		OFFSET2		-2, 0, 0
		SkidWidth	14
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		20, -3, -39,
		OFFSET2		2, 0, 0
		SkidWidth	14
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		20, -17, 21
		LENGTH		17
		DAMPING		2.5
	}


	CoM		0.0 2.0 6.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		39.0

	BODY {
		MASS		1.6f,						; Mass
		INERTIA		1400, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1700, 0.0f, 
					0.0f, 0.0f, 850,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.35
		IsPowered	FALSE

		RADIUS		11
		MASS		0.15					; Mass
		MaxPos		3.0
		STATICFRICTION	1.6					; Static Friction
		KINETICFRICTION	1.4					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	14000

		RADIUS		11
		MASS		0.15					; Mass
		MaxPos		3.0
		STATICFRICTION	1.65				; Static Friction
		KINETICFRICTION	1.45				; Kinetic Friction
		Grip		0.015
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	600.0
		Damping		10.0
		Restitution	-0.85
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	


;/////////////////////////////////////////////////////////////////////
;//
;// Silver single race cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 17: Sgt Bertha Ballistics
;=====================================
Car 17 {

	Name			"Bertha Ballistics"
	Selectable		TRUE
	CLASS			0
	OBTAIN		4
	RATING		2

	EnvRGB	100 100 100

	TPAGE			"cars\sgt\car.bmp"

	COLL			"cars\sgt\hull.hul"

	MODEL	0		"cars\sgt\body.prm"		; Body model
	MODEL	1		"cars\sgt\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\sgt\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\sgt\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\sgt\wheelbr.prm"		; wheel back right
	MODEL	9		"cars\sgt\axle.prm"		; axle
	MODEL	13		"cars\sgt\radar.prm"		; Radar

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-30, -12, 44,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1	    30, -12, 44,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-31, -12, -38
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		31, -12, -38
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		-0, -16, 44
		LENGTH		28
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		0, -16, 44
		LENGTH		28
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		-0, -18, -39
		LENGTH		28
	}
	AXLE 3 {
	    MODELNUM	9
		OFFSET		0, -18, -39
		LENGTH		28
	}

	SPRING 0 - 1 {
		Stiffness	350.0
		Damping		7.0
		Restitution	-0.85
	}

	SPRING 2 - 3 {
		Stiffness	350.0
		Damping		7.0
		Restitution	-0.85
	}

	SPINNER {
		MODELNUM	13
		OFFSET	-24, -61, -20
		AXIS		0, 1.0, 0
		ANGVEL		1.0
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		7, -54, -15
		LENGTH		30
	}

	CoM		0.0 16.0 0.0
	SteerMod	0.4
	SteerRate	8
	TopSpeed	37

	BODY {
		MODELNUM	0
		MASS		3.0
		INERTIA		3000, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 8000, 0.0f, 
					0.0f, 0.0f, 2500,	
	}

	Wheel 0-1 {
		radius	16.0
		IsTurnable	TRUE
		SteerRatio	-0.25
		EngineRatio	30000

		MASS			0.4						; Mass
		MaxPos		15.0
		SkidWidth		12.0
		STATICFRICTION	1.75					; Static Friction
		KINETICFRICTION	1.60					; Kinetic Friction
		Grip		0.015
	}

	Wheel 2-3 {
		radius	18.0
		IsTurnable	TRUE
		SteerRatio	0.03
		EngineRatio	30000

		MASS			0.4						; Mass
		MaxPos		15.0
		SkidWidth		12.0
		STATICFRICTION	1.70					; Static Friction
		KINETICFRICTION	1.60					; Kinetic Friction
		Grip		0.015
	}
}	


;/////////////////////////////////////////////////////////////////////
;//
;// Gold Cup cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 18: Pest Control
;=====================================
Car 18 {

	EnvRGB			200 200 200

	Name			"Pest Control"
	Selectable		TRUE
	CLASS			1
	OBTAIN		1
	RATING		3

	TPAGE			"cars\TC3\car.bmp"

	COLL			"cars\TC3\hull.hul"

	MODEL	0		"cars\TC3\body.prm"			; Body model
	MODEL	1		"cars\TC3\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\TC3\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\TC3\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\TC3\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-22.5, -1, 32.5,
		OFFSET2		-2, 0, 0
		SkidWidth	13
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		22.5, -1, 32.5,
		OFFSET2		2, 0, 0
		SkidWidth	13
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-23, -1, -44.5,
		OFFSET2		-2, 0, 0
		SkidWidth	13
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		23, -1, -44.5,
		OFFSET2		2, 0, 0
		SkidWidth	13
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		20, -22, -44
		LENGTH		17
	}


	CoM		0.0 2.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		47.0

	BODY {
		MASS		2.0f,						; Mass
		INERTIA		1400, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2200, 0.0f, 
					0.0f, 0.0f, 900,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	FALSE

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		5.0
		STATICFRICTION	1.65					; Static Friction
		KINETICFRICTION	1.45					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	18000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		5.0
		STATICFRICTION	1.70					; Static Friction
		KINETICFRICTION	1.50					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	600.0
		Damping		11.0
		Restitution	-0.95
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	


;=====================================
; Car 19: Adeon
;=====================================
Car 19 {

	EnvRGB			200 200 200

	Name			"Adeon"
	Selectable		TRUE
	CLASS			1
	OBTAIN		1
	RATING		3

	TPAGE			"cars\Adeon\car.bmp"

	COLL			"cars\Adeon\hull.hul"

	MODEL	0		"cars\Adeon\body.prm"			; Body model
	MODEL	1		"cars\Adeon\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\Adeon\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\Adeon\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\Adeon\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-23.5, -3, 39,
		OFFSET2		-2, 0, 0
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		23.5, -3, 39,
		OFFSET2		2, 0, 0
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-23.5, -3, -30.5,
		OFFSET2		-2, 0, 0
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		23.5, -3, -30.5,
		OFFSET2		2, 0, 0
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		23, -22, -45
		LENGTH		17
	}


	CoM		0.0 0.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		36.5

	BODY {
		MASS		1.2f,						; Mass
		INERTIA		1000, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1700, 0.0f, 
					0.0f, 0.0f, 560,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	10000

		RADIUS		10
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.80					; Static Friction
		KINETICFRICTION	1.65					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	10000

		RADIUS		10
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.88					; Static Friction
		KINETICFRICTION	1.67					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	1000.0
		Damping		15.0
		Restitution	-0.75
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	


;/////////////////////////////////////////////////////////////////////
;//
;// Gold class practise cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 20: PolePot
;=====================================
Car 20 {

	Name			"Pole Poz"
	Selectable		TRUE
	CLASS			0
	OBTAIN		3
	RATING		3

    EnvRGB  200 200 200

	TPAGE			"cars\fone\car.bmp"

	COLL			"cars\fone\hull.hul"

	MODEL	0		"cars\fone\body.prm"		; Body model
	MODEL	1		"cars\fone\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\fone\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\fone\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\fone\wheelbr.prm"		; wheel back right
	MODEL	9		"cars\fone\axle.prm"		; all axles

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-28, -3, 39,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1	         28, -3, 39,
	        radius          10
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-27, -3, -38,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		27, -3, -38,
	        radius          10
	}

	AXLE 0 {
		MODELNUM	9
		OFFSET		0, -8, 32
		LENGTH		18
	}
	AXLE 1 {
		MODELNUM	9
		OFFSET		0, -8, 32
		LENGTH		18
	}
	AXLE 2 {
		MODELNUM	9
		OFFSET		0, -8, -36
		LENGTH		18
	}
	AXLE 3 {
		MODELNUM	9
		OFFSET		0, -8, -36
		LENGTH		18
	}
	
	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-15, -14, -30
		LENGTH		30
	}

	CoM		0.0 10.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		38.5

	BODY {
		MASS		1.7f,						; Mass
		INERTIA		1100, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2000, 0.0f, 
					0.0f, 0.0f, 1100,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.3
		IsPowered	TRUE
		EngineRatio	13000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		10.0
		STATICFRICTION	1.30					; Static Friction
		KINETICFRICTION	1.15					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	13000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		10.0
		STATICFRICTION	1.33					; Static Friction
		KINETICFRICTION	1.18					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	400.0
		Damping		5.0
		Restitution	-0.90
	}


}	

;=====================================
; Car 21: Zipper
;=====================================
Car 21 {

	EnvRGB			200 200 200

	Name			"Zipper"
	Selectable		TRUE
	CLASS			1
	OBTAIN		3
	RATING		3

	TPAGE			"cars\tc1\car.bmp"
	COLL			"cars\tc1\hull.hul"

	MODEL	0		"cars\tc1\body.prm"			; Body model
	MODEL	1		"cars\tc1\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\tc1\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\tc1\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\tc1\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-21, -4, 34,
		OFFSET2		-2, 0, 0
		SkidWidth	13.5
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		21, -4, 34,
		OFFSET2		2, 0, 0
		SkidWidth	13.5
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-21, -4, -44.5,
		OFFSET2		-2, 0, 0
		SkidWidth	13.5
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		21, -4, -44.5,
		OFFSET2		2, 0, 0
		SkidWidth	13.5
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-22, -18, -45
		LENGTH		17
	}


	CoM		0.0 0.0 5.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		38.0

	BODY {
		MASS		1.4f,						; Mass
		INERTIA		1000, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1700, 0.0f, 
					0.0f, 0.0f, 650,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.4
		IsPowered	TRUE
		EngineRatio	12000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.63					; Static Friction
		KINETICFRICTION	1.45					; Kinetic Friction
		Grip		0.017
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	12000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.65					; Static Friction
		KINETICFRICTION	1.46					; Kinetic Friction
		Grip		0.017
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	700.0
		Damping		9.0
		Restitution	-0.90
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;/////////////////////////////////////////////////////////////////////
;//
;// Gold single race cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 22: WILL BE SPECIAL #1
;=====================================
Car 22 {

	Name			"Rotor"
	Selectable		TRUE
	CLASS			0
	OBTAIN		4
	RATING		3

	EnvRGB			200 200 200

	TPAGE			"cars\rotor\car.bmp"

	COLL			"cars\rotor\hull.hul"

	MODEL	0		"cars\rotor\body.prm"		; Body model
	MODEL	1		"cars\rotor\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\rotor\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\rotor\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\rotor\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	CoM		0.0 9.0 -3.0

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-28, -9.0, 26.5,
		OFFSET2		-13, 0, 0,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1	   28, -9.0, 26.5,
		OFFSET2		13, 0, 0,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-28, -9.0, -27.5
		OFFSET2		-13, 0, 0,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		28, -9.0, -27.5
		OFFSET2		13, 0, 0,
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		0, -27.0, 0
		LENGTH		20
	}

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		10.0
	TopSpeed		45.0

	BODY {
		MODELNUM	0
		MASS		3.0f,						; Mass
		INERTIA		2700, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 3750, 0.0f, 
					0.0f, 0.0f, 2300,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.4
		IsPowered	TRUE
		EngineRatio	38000

		RADIUS		24.5
		MASS			0.45						; Mass
		MaxPos		20.0
		SkidWidth		25.0
		STATICFRICTION	1.70					; Static Friction
		KINETICFRICTION	1.60					; Kinetic Friction
		Grip		0.017
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.03
		IsPowered	TRUE
		EngineRatio	38000

		RADIUS		24.5
		MASS			0.45				; Mass
		MaxPos		20.0
		SkidWidth		25.0
		STATICFRICTION	2.0					; Static Friction
		KINETICFRICTION	1.8					; Kinetic Friction
		Grip		0.017
	}
	SPRING 0-1 {
		Stiffness		1300.0
		Damping		19.2
		Restitution 	-0.95
	}
	SPRING 2-3 {
		Stiffness		1300.0
		Damping		19.2
		Restitution 	-0.95
	}
}	


;/////////////////////////////////////////////////////////////////////
;//
;// Special cup cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 23: Cougar
;=====================================
Car 23 {

	EnvRGB			200 200 200

	Name			"Cougar"
	Selectable		TRUE
	CLASS			1
	OBTAIN		1
	RATING		4

	TPAGE			"cars\Cougar\car.bmp"

	COLL			"cars\Cougar\hull.hul"

	MODEL	0		"cars\Cougar\body.prm"			; Body model
	MODEL	1		"cars\Cougar\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\Cougar\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\Cougar\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\Cougar\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-24.5, -1, 32.5,
		OFFSET2		-1.5, 0, 0
		SkidWidth	11
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		24.5, -1, 32.5,
		OFFSET2		1.5, 0, 0
		SkidWidth	11
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-26.5, -1, -34.5,
		OFFSET2		-1.5, 0, 0
		SkidWidth	12
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		26.5, -1, -34.5,
		OFFSET2		1.5, 0, 0
		SkidWidth	12
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		21, -18, -42
		LENGTH		17
	}


	CoM		0.0 4.0 -10.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		47.0

	BODY {
		MASS		2.0f,						; Mass
		INERTIA		1400, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2200, 0.0f, 
					0.0f, 0.0f, 700,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.18
		IsPowered	TRUE
		EngineRatio	28000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.7					; Static Friction
		KINETICFRICTION	1.65					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	FALSE
		EngineRatio	18000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.73					; Static Friction
		KINETICFRICTION	1.68					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	1000.0
		Damping		15.0
		Restitution	-0.75
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	


;=====================================
; Car 24: Humma
;=====================================
Car 24 {

	EnvRGB			200 200 200

	Name			"Humma"
	Selectable		TRUE
	CLASS			1
	OBTAIN		1
	RATING		4

	TPAGE			"cars\Sugo\car.bmp"

	COLL			"cars\Sugo\hull.hul"

	MODEL	0		"cars\Sugo\body.prm"			; Body model
	MODEL	1		"cars\Sugo\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\Sugo\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\Sugo\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\Sugo\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-23.5, -6, 39,
		OFFSET2		-2, 0, 0
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		23.5, -6, 39,
		OFFSET2		2, 0, 0
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-23.5, -5, -30.5,
		OFFSET2		-2, 0, 0
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		23.5, -5, -30.5,
		OFFSET2		2, 0, 0
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		23, -22, -45
		LENGTH		17
	}


	CoM		0.0 0.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		39.0

	BODY {
		MASS		2.0f,						; Mass
		INERTIA		1400, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2200, 0.0f, 
					0.0f, 0.0f, 700,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	20000

		RADIUS		10
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.72					; Static Friction
		KINETICFRICTION	1.65					; Kinetic Friction
		Grip		0.016
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	20000

		RADIUS		10
		MASS		0.15						; Mass
		MaxPos		3.0
		STATICFRICTION	1.72					; Static Friction
		KINETICFRICTION	1.65					; Kinetic Friction
		Grip		0.016
	}

	SPRING 0 - 1 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	1000.0
		Damping		15.0
		Restitution	-0.85
	}

	SPRING 2 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	800.0
		Damping		12.0
		Restitution	-0.85
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	


;/////////////////////////////////////////////////////////////////////
;//
;// Special practise cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 25: Toyeca
;=====================================
Car 25 {

	EnvRGB			200 200 200

	Name			"Toyeca"
	Selectable		TRUE
	CLASS			1
	OBTAIN		3
	RATING		4

	TPAGE			"cars\Toyeca\Toyecatx.bmp"
	COLL			"cars\Toyeca\hull.hul"

	MODEL	0		"cars\Toyeca\body.prm"			; Body model
	MODEL	1		"cars\Toyeca\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\Toyeca\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\Toyeca\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\Toyeca\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-22.5, -6.75, 35.5,
		OFFSET2		-2.5, 0.0, 0.0,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		22.5, -6.75, 35.5,
		OFFSET2		2.5, 0.0, 0.0,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-24, -6.75, -33,
		OFFSET2		-2, 0.0, 0.0,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		24, -6.75, -33,
		OFFSET2		2, 0.0, 0.0,
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		-17, -22, -45
		LENGTH		17
	}


	CoM		0.0 6.0 -7.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		40.0

	BODY {
		MASS		2.0f,						; Mass
		INERTIA		1400, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 2200, 0.0f, 
					0.0f, 0.0f, 700,	
		GRAVITY		2200.0f,					; Acc due to gravity
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	20000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STEERRATIO	-0.25f						; Steer Ratio
		STATICFRICTION	1.90					; Static Friction
		KINETICFRICTION	1.85					; Kinetic Friction
		Grip		0.018
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	20000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.88					; Static Friction
		KINETICFRICTION	1.85					; Kinetic Friction
		Grip		0.018
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	1000.0
		Damping		15.0
		Restitution	-0.75
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;=====================================
; Car 26: AMW
;=====================================
Car 26 {

	EnvRGB			200 200 200

	Name			"AMW"
	Selectable		TRUE
	CLASS			1
	OBTAIN		3
	RATING		4

	TPAGE			"cars\amw\amw.bmp"

	COLL			"cars\amw\hull.hul"

	MODEL	0		"cars\amw\body.prm"			; Body model
	MODEL	1		"cars\amw\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\amw\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\amw\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\amw\wheelbr.prm"		; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-28.5, -6, 39,
		OFFSET2		-1.5, 0, 0
		SkidWidth	10
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		28.5, -6, 39,
		OFFSET2		1.5, 0, 0
		SkidWidth	10
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-28.5, -6, -29,
		OFFSET2		-1.5, 0, 0
		SkidWidth	10
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		28.5, -6, -29,
		OFFSET2		1.5, 0, 0
		SkidWidth	10
	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		20, -23, 28
		LENGTH		17
	}


	CoM		0.0 6.0 -5.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		40.0

	BODY {
		MASS		1.0f,						; Mass
		INERTIA		700, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1100, 0.0f, 
					0.0f, 0.0f, 350,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	FALSE
		EngineRatio	20000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STEERRATIO	-0.25f						; Steer Ratio
		STATICFRICTION	1.7					; Static Friction
		KINETICFRICTION	1.6					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	21000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		3.0
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.9					; Static Friction
		KINETICFRICTION	1.7					; Kinetic Friction
		Grip		0.014
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	1000.0
		Damping		15.0
		Restitution	-0.75
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;/////////////////////////////////////////////////////////////////////
;//
;// Special class single racs cars
;//
;/////////////////////////////////////////////////////////////////////

;=====================================
; Car 27: WILL BE SPECIAL #2
;=====================================
Car 27 {

	EnvRGB			200 200 200

	Name			"Panga"
	Selectable	TRUE
	CLASS			1
	OBTAIN		3
	RATING		4

	TPAGE			"cars\panga\car.bmp"

	COLL			"cars\panga\hull.hul"

	MODEL	0		"cars\panga\body.prm"			; Body model
	MODEL	1		"cars\panga\wheelfl.prm"			; wheel front left
	MODEL	2		"cars\panga\wheelfr.prm"			; wheel front right
	MODEL	3		"cars\panga\wheelbl.prm"			; wheel back left
	MODEL	4		"cars\panga\wheelbr.prm"			; wheel back right

	MODEL	13		"cars\panga\head.prm"			; head

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-45, 4, 48,
		OFFSET2		-1.5, 0, 0
		SkidWidth	10
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		45, 4, 48,
		OFFSET2		1.5, 0, 0
		SkidWidth	10
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-45, 5, -48,
		OFFSET2		-1.5, 0, 0
		SkidWidth	10
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		45, 5, -48,
		OFFSET2		1.5, 0, 0
		SkidWidth	10
	}

	SPINNER {
		MODELNUM	13
		OFFSET	0, -55, 32
		AXIS		0, 1.0, 0
		ANGVEL		0.0
	}

	CoM		0.0 -10.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		45.0

	BODY {
		MASS		2.5f,						; Mass
		INERTIA	3420, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 4690, 0.0f, 
					0.0f, 0.0f, 2110,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	45000

		RADIUS		22
		MASS		0.15						; Mass
		MaxPos		13.0
		STEERRATIO	-0.25f						; Steer Ratio
		STATICFRICTION	1.7					; Static Friction
		KINETICFRICTION	1.6					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	45000

		RADIUS		26
		MASS		0.15						; Mass
		MaxPos		13.0
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.9					; Static Friction
		KINETICFRICTION	1.7					; Kinetic Friction
		Grip		0.014
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	400.0
		Damping		3.0
		Restitution	-0.95
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	



;/////////////////////////////////////////////////////////////////////
;//
;// Other misc cars
;//
;/////////////////////////////////////////////////////////////////////


;=====================================
; Car 28: Trolley
;=====================================
Car 28 {

	EnvRGB			200 200 200

	Name			"Trolley"
	Selectable		FALSE
	CLASS			2
	OBTAIN		-1
	RATING		4

	TPAGE			NONE ;"models\trolley.bmp"

	COLL			"cars\trolley\trolleyHull.hul"

	MODEL	0		"cars\trolley\TrollBod.m"			; Body model
	MODEL	1		"cars\trolley\TrollWL.m"			; wheel front left
	MODEL	2		"cars\trolley\TrollWR.m"			; wheel front right
	MODEL	3		"cars\trolley\TrollWL.m"			; wheel back left
	MODEL	4		"cars\trolley\TrollWR.m"			; wheel back right

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top

	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-50, 10, 110,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		50, 10, 110,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-70, 10, -100,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		70, 10, -100,
	}


	CoM		0.0 80.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		40.0

	BODY {
		MASS		10.0f,						; Mass
		INERTIA		20000, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 22000, 0.0f, 
					0.0f, 0.0f, 12000,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	FALSE
		EngineRatio	20000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		10.0
		STEERRATIO	-0.5f						; Steer Ratio
		STATICFRICTION	1.9					; Static Friction
		KINETICFRICTION	1.7					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	20000

		RADIUS		11
		MASS		0.15						; Mass
		MaxPos		10.0
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.9					; Static Friction
		KINETICFRICTION	1.7					; Kinetic Friction
		Grip		0.015
	}

	SPRING 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0,
		Stiffness	500.0
		Damping		10.0
		Restitution	-0.75
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}	

;=====================================
; Car 29: key car
;=====================================
Car 29 {

	Name			"Cockwork"
	Selectable		TRUE
	CLASS			0
	OBTAIN		-1
	RATING		4

	EnvRGB	255 255 255

	TPAGE			"cars\wincar\car.bmp"

	COLL			"cars\wincar\hull.hul"

	MODEL	0		"cars\wincar\body.prm"			; Body model
	MODEL	1		"cars\wincar\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\wincar\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\wincar\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\wincar\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\wincar\key.prm"			; spinny key

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top



	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-14, 0, 22,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		14, 0, 22,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-14, 0, -22,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		14, 0, -22,
	}

	SPINNER {
		MODELNUM	5
		OFFSET	0, 0, 0
		AXIS		0, 1.0, 0
		ANGVEL		-0.5
	}

	CoM		0.0 12.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		34.0

	BODY {
		MASS		1.2f,						; Mass
		INERTIA		1200, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1800, 0.0f, 
					0.0f, 0.0f, 650,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	3500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO	-0.5f						; Steer Ratio
		STATICFRICTION	1.1					; Static Friction
		KINETICFRICTION	0.9					; Kinetic Friction
		Grip		0.011
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	3500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.1					; Static Friction
		KINETICFRICTION	0.9					; Kinetic Friction
		Grip		0.011
	}

	SPRING 0-1 {
		Stiffness	500.0
		Damping		12.0
		Restitution	-0.8
	}
	SPRING 2-3 {
		Stiffness	460.0
		Damping		10.0
		Restitution	-0.8
	}

}	

;=====================================
; Car 30: key car 2
;=====================================
Car 30 {

	Name			"Cockwork Too"
	Selectable		TRUE
	CLASS			0
	OBTAIN		-1
	RATING		4

	EnvRGB	200 200 0

	TPAGE			"cars\wincar2\car.bmp"

	COLL			"cars\wincar2\hull.hul"

	MODEL	0		"cars\wincar2\body.prm"			; Body model
	MODEL	1		"cars\wincar2\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\wincar2\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\wincar2\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\wincar2\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\wincar2\key.prm"			; spinny key

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top


	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-14, 0, 22,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		14, 0, 22,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-14, 0, -22,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		14, 0, -22,
	}

	SPINNER {
		MODELNUM	5
		OFFSET	0, 9, 0
		AXIS		0, 1.0, 0
		ANGVEL		-0.5
	}

	CoM		0.0 12.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		34.0

	BODY {
		MASS		1.2f,						; Mass
		INERTIA		1200, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1800, 0.0f, 
					0.0f, 0.0f, 650,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	3500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO	-0.5f						; Steer Ratio
		STATICFRICTION	1.1					; Static Friction
		KINETICFRICTION	0.9					; Kinetic Friction
		Grip		0.011
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	3500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.1					; Static Friction
		KINETICFRICTION	0.9					; Kinetic Friction
		Grip		0.011
	}

	SPRING 0-1 {
		Stiffness	500.0
		Damping		12.0
		Restitution	-0.8
	}
	SPRING 2-3 {
		Stiffness	460.0
		Damping		10.0
		Restitution	-0.8
	}

}	

;=====================================
; Car 31: key car 3
;=====================================
Car 31 {

	Name			"Cockwork Tree"
	Selectable		TRUE
	CLASS			0
	OBTAIN		-1
	RATING		4

	EnvRGB	200 200 0

	TPAGE			"cars\wincar3\car.bmp"

	COLL			"cars\wincar3\hull.hul"

	MODEL	0		"cars\wincar3\body.prm"			; Body model
	MODEL	1		"cars\wincar3\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\wincar3\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\wincar3\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\wincar3\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\wincar3\key.prm"			; spinny key

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top


	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-14, 0, 22,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		14, 0, 22,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-14, 0, -22,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		14, 0, -22,
	}

	SPINNER {
		MODELNUM	5
		OFFSET	0, 21, 0
		AXIS		0, 1.0, 0
		ANGVEL		-0.5
	}

	CoM		0.0 12.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		34.0

	BODY {
		MASS		1.2f,						; Mass
		INERTIA		1200, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1800, 0.0f, 
					0.0f, 0.0f, 650,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	3500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO	-0.5f						; Steer Ratio
		STATICFRICTION	1.1					; Static Friction
		KINETICFRICTION	0.9					; Kinetic Friction
		Grip		0.011
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	3500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.1					; Static Friction
		KINETICFRICTION	0.9					; Kinetic Friction
		Grip		0.011
	}

	SPRING 0-1 {
		Stiffness	500.0
		Damping		12.0
		Restitution	-0.8
	}
	SPRING 2-3 {
		Stiffness	460.0
		Damping		10.0
		Restitution	-0.8
	}

}	


;=====================================
; Car 32: key car 4
;=====================================
Car 32 {

	Name			"Cockwork"
	Selectable		TRUE
	CLASS			0
	OBTAIN		-1
	RATING		4

	EnvRGB		255 255 255

	TPAGE			"cars\wincar4\car.bmp"

	COLL			"cars\wincar4\hull.hul"

	MODEL	0		"cars\wincar4\body.prm"			; Body model
	MODEL	1		"cars\wincar4\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\wincar4\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\wincar4\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\wincar4\wheelbr.prm"		; wheel back right
	MODEL	5		"cars\wincar4\key.prm"			; spinny key

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top


	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-14, 0, 22,
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		14, 0, 22,
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-14, 0, -22,
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		14, 0, -22,
	}

	SPINNER {
		MODELNUM	5
		OFFSET	0, 21, 0
		AXIS		0, 1.0, 0
		ANGVEL		-0.5
	}

	CoM		0.0 0.0 0.0

	SteerRate	3.0
	SteerMod		0.4
	EngineRate	4.5
	TopSpeed		45.0

	BODY {
		MASS		1.2f,							; Mass
		INERTIA	1200, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1800, 0.0f, 
					0.0f, 0.0f, 650,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		IsPowered	TRUE
		EngineRatio	7500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO	-0.5f					; Steer Ratio
		STATICFRICTION	2.0				; Static Friction
		KINETICFRICTION	1.8				; Kinetic Friction
		Grip		0.014
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		IsPowered	TRUE
		EngineRatio	7500

		RADIUS		9
		MASS		0.15						; Mass
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	2.0					; Static Friction
		KINETICFRICTION	1.8					; Kinetic Friction
		Grip		0.014
	}

	SPRING 0-1 {
		Stiffness	500.0
		Damping		12.0
		Restitution	-0.8
	}
	SPRING 2-3 {
		Stiffness	460.0
		Damping		10.0
		Restitution	-0.8
	}

}	


;=====================================
; Car 33: UFO
;=====================================
Car 33 {

	Name			"Probe UFO"
	Selectable		FALSE
	CLASS			0
	OBTAIN		-1
	RATING		0

	EnvRGB	255 255 255

	TPAGE			"cars\UFO\car.bmp"

	COLL			"cars\UFO\hull.hul"

	MODEL	0		"cars\UFO\body.prm"			; Body model
	MODEL	1		"cars\UFO\wheelfl.prm"		; wheel front left
	MODEL	2		"cars\UFO\wheelfr.prm"		; wheel front right
	MODEL	3		"cars\UFO\wheelbl.prm"		; wheel back left
	MODEL	4		"cars\UFO\wheelbr.prm"		; wheel back right
	; MODEL	5		"cars\UFO\axlefl.prm"
	; MODEL	6		"cars\UFO\axlefr.prm"
	; MODEL	7		"cars\UFO\axlebl.prm"
	; MODEL	8		"cars\UFO\axlebr.prm"

	MODEL	17		"cars\misc\Aerial.m"		; Aerial section
	MODEL	18		"cars\misc\AerialT.m"		; Aerial Top


	BODY {
		MODELNUM	0
	}

	WHEEL 0 {
		MODELNUM	1
		OFFSET1		-20, 35, 20,
		OFFSET2		-0.5, 0, 0
		SkidWidth	6
	}
	WHEEL 1 {
		MODELNUM	2
		OFFSET1		20, 35, 20,
		OFFSET2		0.5, 0, 0
		SkidWidth	6
	}
	WHEEL 2 {
		MODELNUM	3
		OFFSET1		-20, 35, -20,
		OFFSET2		-0.5, 0, 0
		SkidWidth	6
	}
	WHEEL 3 {
		MODELNUM	4
		OFFSET1		20, 35, -20,
		OFFSET2		0.5, 0, 0
		SkidWidth	6
	}

;	SPRING 0 {
; 		MODELNUM		4
; 		OFFSET		-20, 45, 20,
; 		LENGTH		13
; 	}
; 	SPRING 1 {
; 		MODELNUM		4
; 		OFFSET		20, 45, 20,
; 		LENGTH		13
; 	}
; 	SPRING 2 {
; 		MODELNUM		4
; 		OFFSET		-20, 45, -20,
; 		LENGTH		13
; 	}
; 	SPRING 3 {
; 		MODELNUM		4
; 		OFFSET		20, 45, -20,
; 		LENGTH		13
; 	}

	AERIAL {
		SECMODELNUM	17
		TOPMODELNUM 18
		OFFSET		0, -13, 0
		LENGTH		17
	}


	CoM		0.0 -20.0 0.0

	SteerRate		3.0
	SteerMod		0.4
	EngineRate		4.5
	TopSpeed		40.0

	BODY {
		MASS		1.0f,						; Mass 
		INERTIA		700, 0.0f, 0.0f,			; Inertia Matrix (MUST BE SYMMETRIC)
					0.0f, 1100, 0.0f, 
					0.0f, 0.0f, 350,	
	}

	WHEEL 0-1 {
		IsTurnable	TRUE
		SteerRatio	-0.5
		IsPowered	TRUE
		EngineRatio	10000

		RADIUS		6
		MASS		0.15						; Mass
		MaxPos		3.0
		STEERRATIO	-0.25f						; Steer Ratio
		STATICFRICTION	1.0					; Static Friction
		KINETICFRICTION	0.7					; Kinetic Friction
		Grip		0.015
	}
	WHEEL 2-3 {
		IsTurnable	FALSE
		SteerRatio	0.0
		IsPowered	TRUE
		EngineRatio	10000

		RADIUS		6
		MASS		0.15						; Mass
		MaxPos		3.0
		STEERRATIO		1.0f					; Steer Ratio
		STATICFRICTION	1.0					; Static Friction
		KINETICFRICTION	0.7					; Kinetic Friction
		Grip		0.014
	}

	SPRING 0 - 3 {
		Stiffness	500.0
		Damping		6.0
		Restitution	-0.90
	}

	PIN 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}

	AXLE 0 - 3 {
		MODELNUM	-1
		OFFSET		0, 0, 0,
		LENGTH		0, 
	}
}
4A4641C8